Unchangeable Pins:

* I2C\_0 SCL: 9
* I2C\_0 SDA: 10
* I2C\_1 SCL: 14
* I2C\_1 SDA: 15
* RX: 3
* TX: 4

Changeable Pins:

* PM\_SLEEP\_PIN: 6
* CO2\_SLEEP\_PIN: 7
* ANEM\_SLEEP\_PIN: 8
* ULTRASONIC\_TRIG\_1: 16
* ULTRASONIC\_ECHO\_1: 17
* ULTRASONIC\_TRIG\_2: 18
* ULTRASONIC\_ECHO\_2: 19
* Manny please put changeable smartmesh pins here

Notes:

* Sleep pins should have spots for transistors to turn off that sensor. Not likely to need them all, but probably nice to have
* Likely will need 2nd I2C bus for just CO2 sensor in order to properly put it to sleep without messing with other sensors on bus



